Cisco UCS As Built Documentation

ConvergeOne

|  |  |
| --- | --- |
| Author: | BWetteroff |
| Date: | 21 March 2019 |
| Version: | 2 |

# 1 Cluster Status

|  |  |
| --- | --- |
| Name | UCSPE-192-168-2-115 |
| Virtual IP Address | 192.168.2.115 |
| HA Configuration | cluster |
| HA Readiness | ready |
| HA Ready | yes |
| Ethernet State | full |

|  |  |
| --- | --- |
| Fabric Interconnect A Role | primary |
| Fabric Interconnect A IP Address | 192.168.2.116 |
| Fabric Interconnect A Subnet Mask | 255.255.255.0 |
| Fabric Interconnect A Default Gateway | 192.168.2.1 |
| Fabric Interconnect A State | up |

|  |  |
| --- | --- |
| Fabric Interconnect B Role | subordinate |
| Fabric Interconnect B IP Address | 192.168.2.117 |
| Fabric Interconnect B Subnet Mask | 255.255.255.0 |
| Fabric Interconnect B Default Gateway | 192.168.2.1 |
| Fabric Interconnect B State | up |

# 2 Equipment

## 2.1 Chassis

### 2.1.1 Chassis Inventory

|  |  |
| --- | --- |
| Chassis | chassis-1 |
| Model | UCSB-5108-AC2 |
| Admin State | acknowledged |
| Operability | operable |
| License State | license-ok |
| Power | ok |
| Thermal | ok |
| Serial | CH39 |

|  |  |
| --- | --- |
| Chassis | chassis-2 |
| Model | UCSC-C3X60-BASE |
| Admin State | acknowledged |
| Operability | power-problem |
| License State | license-ok |
| Power | input-failed |
| Thermal | unknown |
| Serial | CH40 |

|  |  |
| --- | --- |
| Chassis | chassis-3 |
| Model | UCSB-5108-AC2 |
| Admin State | acknowledged |
| Operability | operable |
| License State | license-ok |
| Power | ok |
| Thermal | ok |
| Serial | CH43 |

|  |  |
| --- | --- |
| Chassis | chassis-4 |
| Model | UCSC-C3X60-BASE |
| Admin State | acknowledged |
| Operability | power-problem |
| License State | license-ok |
| Power | input-failed |
| Thermal | unknown |
| Serial | CH44 |

### 2.1.2 IOM Inventory

| Chassis Id | Relative Name | Model | Discovery | Configuration State | Operability | Side | Thermal | Serial |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1 | slot-1 | UCS-IOM-2304 | online | ok | operable | left | ok | IOM37 |
| 1 | slot-2 | UCS-IOM-2304 | online | ok | operable | right | ok | IOM38 |
| 3 | slot-1 | UCS-IOM-2304 | online | ok | operable | left | ok | IOM43 |
| 3 | slot-2 | UCS-IOM-2304 | online | ok | operable | right | ok | IOM44 |

### 2.1.3 Fabric Interconnect to IOM Connections

| Chassis Id | Discovery | Model | Operability | Switch Id | Peer Slot Id | Peer Port Id | Sloy Id | Port Id | XcvrType |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1 | present | UCS-IOM-2304 | up | A | 1 | 25 | 1 | 1 | unknown |
| 1 | present | UCS-IOM-2304 | up | A | 1 | 26 | 1 | 2 | unknown |
| 1 | present | UCS-IOM-2304 | up | A | 1 | 27 | 1 | 3 | unknown |
| 1 | present | UCS-IOM-2304 | up | A | 1 | 28 | 1 | 4 | unknown |
| 1 | present | UCS-IOM-2304 | up | B | 1 | 25 | 2 | 1 | unknown |
| 1 | present | UCS-IOM-2304 | up | B | 1 | 26 | 2 | 2 | unknown |
| 1 | present | UCS-IOM-2304 | up | B | 1 | 27 | 2 | 3 | unknown |
| 1 | present | UCS-IOM-2304 | up | B | 1 | 28 | 2 | 4 | unknown |
| 2 | present | UCSC-C3X60-BASE | up | A | 1 | 21 | 1 | 1 | unknown |
| 2 | present | UCSC-C3X60-BASE | up | B | 1 | 21 | 1 | 5 | unknown |
| 2 | present | UCSC-C3X60-BASE | up | A | 1 | 22 | 2 | 1 | unknown |
| 2 | present | UCSC-C3X60-BASE | up | B | 1 | 22 | 2 | 5 | unknown |
| 3 | present | UCS-IOM-2304 | up | A | 1 | 17 | 1 | 1 | unknown |
| 3 | present | UCS-IOM-2304 | up | A | 1 | 18 | 1 | 2 | unknown |
| 3 | present | UCS-IOM-2304 | up | A | 1 | 19 | 1 | 3 | unknown |
| 3 | present | UCS-IOM-2304 | up | A | 1 | 20 | 1 | 4 | unknown |
| 3 | present | UCS-IOM-2304 | up | B | 1 | 17 | 2 | 1 | unknown |
| 3 | present | UCS-IOM-2304 | up | B | 1 | 18 | 2 | 2 | unknown |
| 3 | present | UCS-IOM-2304 | up | B | 1 | 19 | 2 | 3 | unknown |
| 3 | present | UCS-IOM-2304 | up | B | 1 | 20 | 2 | 4 | unknown |
| 4 | present | UCSC-C3X60-BASE | up | A | 1 | 23 | 1 | 1 | unknown |
| 4 | present | UCSC-C3X60-BASE | up | B | 1 | 23 | 1 | 5 | unknown |
| 4 | present | UCSC-C3X60-BASE | up | A | 1 | 24 | 2 | 1 | unknown |
| 4 | present | UCSC-C3X60-BASE | up | B | 1 | 24 | 2 | 5 | unknown |

### 2.1.4 Chassis Discovery Policy

| Ucs | Relative Name | Link Aggregation Preference | Action |
| --- | --- | --- | --- |
| UCSPE-192-168-2-115 | chassis-discovery | none | 1-link |

### 2.1.5 Chassis Power Policy

| Ucs | Relative Name | Redundancy |
| --- | --- | --- |
| UCSPE-192-168-2-115 | psu-policy | n+1 |

### 2.1.6 Blade Server Inventory

| Server Id | Model | Available Memory | Number of CPUs | Number of Cores | Number of Adapters | Number of Ethernet Interfaces | Number of FC Host Interfaces | Assigned To | Presence | Operability | Power | Serial |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1/1 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV127 |
| 1/2 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV135 |
| 1/3 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV136 |
| 1/4 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV137 |
| 1/5 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV138 |
| 1/6 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV139 |
| 1/7 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV140 |
| 1/8 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV141 |
| 2/1 | UCSC-C3K-M4SRB | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV111 |
| 2/2 | UCSC-C3K-M4SRB | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV112 |
| 3/1 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV142 |
| 3/2 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV143 |
| 3/3 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV144 |
| 3/4 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV145 |
| 3/5 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV146 |
| 3/6 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV147 |
| 3/7 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV148 |
| 3/8 | UCSB-B200-M5 | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV149 |
| 4/1 | UCSC-C3K-M4SRB | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV150 |
| 4/2 | UCSC-C3K-M4SRB | 49152 | 2 | 8 | 1 | 0 | 0 |  | equipped | unassociated | off | SRV151 |

### 2.1.7 Server Adaptor Inventory

| Chassis Id | Blade Id | Relative Name | Model |
| --- | --- | --- | --- |
| 1 | 1 | adaptor-1 | UCSB-MLOM-40G-03 |
| 1 | 2 | adaptor-1 | UCSB-MLOM-40G-03 |
| 1 | 3 | adaptor-1 | UCSB-MLOM-40G-03 |
| 1 | 4 | adaptor-1 | UCSB-MLOM-40G-03 |
| 1 | 5 | adaptor-1 | UCSB-MLOM-40G-03 |
| 1 | 6 | adaptor-1 | UCSB-MLOM-40G-03 |
| 1 | 7 | adaptor-1 | UCSB-MLOM-40G-03 |
| 1 | 8 | adaptor-1 | UCSB-MLOM-40G-03 |
| 2 | 1 | adaptor-1 | UCSC-C3260-SIOC |
| 2 | 2 | adaptor-2 | UCSC-C3260-SIOC |
| 3 | 1 | adaptor-1 | UCSB-MLOM-40G-03 |
| 3 | 2 | adaptor-1 | UCSB-MLOM-40G-03 |
| 3 | 3 | adaptor-1 | UCSB-MLOM-40G-03 |
| 3 | 4 | adaptor-1 | UCSB-MLOM-40G-03 |
| 3 | 5 | adaptor-1 | UCSB-MLOM-40G-03 |
| 3 | 6 | adaptor-1 | UCSB-MLOM-40G-03 |
| 3 | 7 | adaptor-1 | UCSB-MLOM-40G-03 |
| 3 | 8 | adaptor-1 | UCSB-MLOM-40G-03 |
| 4 | 1 | adaptor-1 | UCSC-C3260-SIOC |
| 4 | 2 | adaptor-2 | UCSC-C3260-SIOC |

### 2.1.8 Server CPU Inventory

| Distinguished Name | Socket Designation | Cores | Cores Enabled | Threads | Speed | Operability | Thermal | Model |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| sys/chassis-1/blade-1/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-1/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-2/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-2/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-3/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-3/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-4/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-4/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-5/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-5/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-6/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-6/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-7/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-7/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-8/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-1/blade-8/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-2/blade-1/board/cpu-1 | CPU1 | 4 | 4 | 8 | 2.400000 | operable | ok | Intel(R) Xeon(R) CPU E5-2680 v4 @ 2.40GHz |
| sys/chassis-2/blade-1/board/cpu-2 | CPU2 | 4 | 4 | 8 | 2.400000 | operable | ok | Intel(R) Xeon(R) CPU E5-2680 v4 @ 2.40GHz |
| sys/chassis-2/blade-2/board/cpu-1 | CPU1 | 4 | 4 | 8 | 2.400000 | operable | ok | Intel(R) Xeon(R) CPU E5-2680 v4 @ 2.40GHz |
| sys/chassis-2/blade-2/board/cpu-2 | CPU2 | 4 | 4 | 8 | 2.400000 | operable | ok | Intel(R) Xeon(R) CPU E5-2680 v4 @ 2.40GHz |
| sys/chassis-3/blade-1/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-1/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-2/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-2/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-3/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-3/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-4/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-4/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-5/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-5/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-6/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-6/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-7/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-7/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-8/board/cpu-1 | CPU1 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-3/blade-8/board/cpu-2 | CPU2 | 4 | 4 | 8 | 3.200000 | operable | ok | Intel(R) Xeon(R) CPU E7-8893 v3 @ 3.20GHz |
| sys/chassis-4/blade-1/board/cpu-1 | CPU1 | 4 | 4 | 8 | 2.400000 | operable | ok | Intel(R) Xeon(R) CPU E5-2680 v4 @ 2.40GHz |
| sys/chassis-4/blade-1/board/cpu-2 | CPU2 | 4 | 4 | 8 | 2.400000 | operable | ok | Intel(R) Xeon(R) CPU E5-2680 v4 @ 2.40GHz |
| sys/chassis-4/blade-2/board/cpu-1 | CPU1 | 4 | 4 | 8 | 2.400000 | operable | ok | Intel(R) Xeon(R) CPU E5-2680 v4 @ 2.40GHz |
| sys/chassis-4/blade-2/board/cpu-2 | CPU2 | 4 | 4 | 8 | 2.400000 | operable | ok | Intel(R) Xeon(R) CPU E5-2680 v4 @ 2.40GHz |

### 2.1.9 Server Memory Inventory

| Distinguished Name | Location | Capacity | Clock | Operability | Model |
| --- | --- | --- | --- | --- | --- |
| sys/chassis-1/blade-1/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-1/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-2/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-3/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-4/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-5/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-6/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-7/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-1/blade-8/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-2/blade-1/board/memarray-1/mem-1 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-10 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-11 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-12 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-13 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-14 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-15 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-16 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-2 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-3 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-4 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-5 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-6 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-7 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-8 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-1/board/memarray-1/mem-9 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-1 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-10 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-11 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-12 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-13 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-14 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-15 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-16 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-2 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-3 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-4 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-5 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-6 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-7 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-8 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-2/blade-2/board/memarray-1/mem-9 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-3/blade-1/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-1/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-2/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-3/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-4/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-5/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-6/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-7/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-1 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-10 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-11 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-12 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-13 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-14 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-15 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-16 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-17 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-18 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-19 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-2 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-20 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-21 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-22 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-23 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-24 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-3 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-4 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-5 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-6 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-7 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-8 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-3/blade-8/board/memarray-1/mem-9 |  | 32768 | 2133 | operable | HMA84GR7MFR4N-TFTD |
| sys/chassis-4/blade-1/board/memarray-1/mem-1 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-10 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-11 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-12 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-13 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-14 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-15 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-16 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-2 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-3 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-4 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-5 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-6 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-7 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-8 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-1/board/memarray-1/mem-9 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-1 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-10 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-11 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-12 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-13 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-14 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-15 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-16 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-2 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-3 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-4 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-5 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-6 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-7 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-8 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |
| sys/chassis-4/blade-2/board/memarray-1/mem-9 |  | 32768 | 2400 | operable | 36ASF4G72PZ-2G3B1 |

### 2.1.10 Server Storage Controller Inventory

| Vendor | Model |
| --- | --- |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| Intel Corp. | Patsburg Dual 4-Port SATA SAS Storage Control Unit SKU ROM 5 |
| Cisco Systems Inc | UCS-C3K-M4RAID |
| Intel Corp. | Patsburg Dual 4-Port SATA SAS Storage Control Unit SKU ROM 5 |
| Cisco Systems Inc | UCS-C3K-M4RAID |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| LSI Corp. | LSI 6G MegaRAID SAS 9266-8i |
| Intel Corp. | Patsburg Dual 4-Port SATA SAS Storage Control Unit SKU ROM 5 |
| Cisco Systems Inc | UCS-C3K-M4RAID |
| Intel Corp. | Patsburg Dual 4-Port SATA SAS Storage Control Unit SKU ROM 5 |
| Cisco Systems Inc | UCS-C3K-M4RAID |

### 2.1.11 Server Local Disk Inventory

| Distinguished Name | Model | Size | Serial |
| --- | --- | --- | --- |
| sys/chassis-2/blade-1/enc-3/disk-201 | INTEL SSDSC2BB120G6K1 | 114473 | SRVDISK224 |
| sys/chassis-2/blade-1/enc-3/disk-202 | INTEL SSDSC2BB120G6K1 | 114473 | SRVDISK225 |
| sys/chassis-2/blade-2/enc-3/disk-201 | INTEL SSDSC2BB120G6K1 | 114473 | SRVDISK226 |
| sys/chassis-2/blade-2/enc-3/disk-202 | INTEL SSDSC2BB120G6K1 | 114473 | SRVDISK227 |
| sys/chassis-2/enc-1/disk-1 | HUS726060AL4210 | not-applicable | CHDISK670 |
| sys/chassis-2/enc-1/disk-10 | HUS726060AL4210 | not-applicable | CHDISK679 |
| sys/chassis-2/enc-1/disk-11 | HUS726060AL4210 | not-applicable | CHDISK680 |
| sys/chassis-2/enc-1/disk-12 | HUS726060AL4210 | not-applicable | CHDISK681 |
| sys/chassis-2/enc-1/disk-13 | HUS726060AL4210 | not-applicable | CHDISK682 |
| sys/chassis-2/enc-1/disk-14 | HUS726060AL4210 | not-applicable | CHDISK683 |
| sys/chassis-2/enc-1/disk-15 | HUS726060AL4210 | not-applicable | CHDISK684 |
| sys/chassis-2/enc-1/disk-16 | HUS726060AL4210 | not-applicable | CHDISK685 |
| sys/chassis-2/enc-1/disk-17 | HUS726060AL4210 | not-applicable | CHDISK686 |
| sys/chassis-2/enc-1/disk-18 | HUS726060AL4210 | not-applicable | CHDISK687 |
| sys/chassis-2/enc-1/disk-19 | HUS726060AL4210 | not-applicable | CHDISK688 |
| sys/chassis-2/enc-1/disk-2 | HUS726060AL4210 | not-applicable | CHDISK671 |
| sys/chassis-2/enc-1/disk-20 | HUS726060AL4210 | not-applicable | CHDISK689 |
| sys/chassis-2/enc-1/disk-21 | HUS726060AL4210 | not-applicable | CHDISK690 |
| sys/chassis-2/enc-1/disk-22 | HUS726060AL4210 | not-applicable | CHDISK691 |
| sys/chassis-2/enc-1/disk-23 | HUS726060AL4210 | not-applicable | CHDISK692 |
| sys/chassis-2/enc-1/disk-24 | HUS726060AL4210 | not-applicable | CHDISK693 |
| sys/chassis-2/enc-1/disk-25 | HUS726060AL4210 | not-applicable | CHDISK694 |
| sys/chassis-2/enc-1/disk-26 | HUS726060AL4210 | not-applicable | CHDISK695 |
| sys/chassis-2/enc-1/disk-27 | HUS726060AL4210 | not-applicable | CHDISK696 |
| sys/chassis-2/enc-1/disk-28 | HUS726060AL4210 | not-applicable | CHDISK697 |
| sys/chassis-2/enc-1/disk-29 | HUS726060AL4210 | not-applicable | CHDISK698 |
| sys/chassis-2/enc-1/disk-3 | HUS726060AL4210 | not-applicable | CHDISK672 |
| sys/chassis-2/enc-1/disk-30 | HUS726060AL4210 | not-applicable | CHDISK699 |
| sys/chassis-2/enc-1/disk-31 | HUS726060AL4210 | not-applicable | CHDISK700 |
| sys/chassis-2/enc-1/disk-32 | HUS726060AL4210 | not-applicable | CHDISK701 |
| sys/chassis-2/enc-1/disk-33 | HUS726060AL4210 | not-applicable | CHDISK702 |
| sys/chassis-2/enc-1/disk-34 | HUS726060AL4210 | not-applicable | CHDISK703 |
| sys/chassis-2/enc-1/disk-35 | HUS726060AL4210 | not-applicable | CHDISK704 |
| sys/chassis-2/enc-1/disk-36 | HUS726060AL4210 | not-applicable | CHDISK705 |
| sys/chassis-2/enc-1/disk-37 | HUS726060AL4210 | not-applicable | CHDISK706 |
| sys/chassis-2/enc-1/disk-38 | HUS726060AL4210 | not-applicable | CHDISK707 |
| sys/chassis-2/enc-1/disk-39 | HUS726060AL4210 | not-applicable | CHDISK708 |
| sys/chassis-2/enc-1/disk-4 | HUS726060AL4210 | not-applicable | CHDISK673 |
| sys/chassis-2/enc-1/disk-40 | HUS726060AL4210 | not-applicable | CHDISK709 |
| sys/chassis-2/enc-1/disk-41 | HUS726060AL4210 | not-applicable | CHDISK710 |
| sys/chassis-2/enc-1/disk-42 | HUS726060AL4210 | not-applicable | CHDISK711 |
| sys/chassis-2/enc-1/disk-43 | HUS726060AL4210 | not-applicable | CHDISK712 |
| sys/chassis-2/enc-1/disk-44 | HUS726060AL4210 | not-applicable | CHDISK713 |
| sys/chassis-2/enc-1/disk-45 | HUS726060AL4210 | not-applicable | CHDISK714 |
| sys/chassis-2/enc-1/disk-46 | HUS726060AL4210 | not-applicable | CHDISK715 |
| sys/chassis-2/enc-1/disk-47 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK716 |
| sys/chassis-2/enc-1/disk-48 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK717 |
| sys/chassis-2/enc-1/disk-49 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK718 |
| sys/chassis-2/enc-1/disk-5 | HUS726060AL4210 | not-applicable | CHDISK674 |
| sys/chassis-2/enc-1/disk-50 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK719 |
| sys/chassis-2/enc-1/disk-51 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK720 |
| sys/chassis-2/enc-1/disk-52 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK721 |
| sys/chassis-2/enc-1/disk-53 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK722 |
| sys/chassis-2/enc-1/disk-54 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK723 |
| sys/chassis-2/enc-1/disk-55 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK724 |
| sys/chassis-2/enc-1/disk-56 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK725 |
| sys/chassis-2/enc-1/disk-6 | HUS726060AL4210 | not-applicable | CHDISK675 |
| sys/chassis-2/enc-1/disk-7 | HUS726060AL4210 | not-applicable | CHDISK676 |
| sys/chassis-2/enc-1/disk-8 | HUS726060AL4210 | not-applicable | CHDISK677 |
| sys/chassis-2/enc-1/disk-9 | HUS726060AL4210 | not-applicable | CHDISK678 |
| sys/chassis-4/blade-1/enc-3/disk-201 | INTEL SSDSC2BB120G6K1 | 114473 | SRVDISK256 |
| sys/chassis-4/blade-1/enc-3/disk-202 | INTEL SSDSC2BB120G6K1 | 114473 | SRVDISK257 |
| sys/chassis-4/blade-2/enc-3/disk-201 | INTEL SSDSC2BB120G6K1 | 114473 | SRVDISK258 |
| sys/chassis-4/blade-2/enc-3/disk-202 | INTEL SSDSC2BB120G6K1 | 114473 | SRVDISK259 |
| sys/chassis-4/enc-1/disk-1 | HUS726060AL4210 | not-applicable | CHDISK726 |
| sys/chassis-4/enc-1/disk-10 | HUS726060AL4210 | not-applicable | CHDISK735 |
| sys/chassis-4/enc-1/disk-11 | HUS726060AL4210 | not-applicable | CHDISK736 |
| sys/chassis-4/enc-1/disk-12 | HUS726060AL4210 | not-applicable | CHDISK737 |
| sys/chassis-4/enc-1/disk-13 | HUS726060AL4210 | not-applicable | CHDISK738 |
| sys/chassis-4/enc-1/disk-14 | HUS726060AL4210 | not-applicable | CHDISK739 |
| sys/chassis-4/enc-1/disk-15 | HUS726060AL4210 | not-applicable | CHDISK740 |
| sys/chassis-4/enc-1/disk-16 | HUS726060AL4210 | not-applicable | CHDISK741 |
| sys/chassis-4/enc-1/disk-17 | HUS726060AL4210 | not-applicable | CHDISK742 |
| sys/chassis-4/enc-1/disk-18 | HUS726060AL4210 | not-applicable | CHDISK743 |
| sys/chassis-4/enc-1/disk-19 | HUS726060AL4210 | not-applicable | CHDISK744 |
| sys/chassis-4/enc-1/disk-2 | HUS726060AL4210 | not-applicable | CHDISK727 |
| sys/chassis-4/enc-1/disk-20 | HUS726060AL4210 | not-applicable | CHDISK745 |
| sys/chassis-4/enc-1/disk-21 | HUS726060AL4210 | not-applicable | CHDISK746 |
| sys/chassis-4/enc-1/disk-22 | HUS726060AL4210 | not-applicable | CHDISK747 |
| sys/chassis-4/enc-1/disk-23 | HUS726060AL4210 | not-applicable | CHDISK748 |
| sys/chassis-4/enc-1/disk-24 | HUS726060AL4210 | not-applicable | CHDISK749 |
| sys/chassis-4/enc-1/disk-25 | HUS726060AL4210 | not-applicable | CHDISK750 |
| sys/chassis-4/enc-1/disk-26 | HUS726060AL4210 | not-applicable | CHDISK751 |
| sys/chassis-4/enc-1/disk-27 | HUS726060AL4210 | not-applicable | CHDISK752 |
| sys/chassis-4/enc-1/disk-28 | HUS726060AL4210 | not-applicable | CHDISK753 |
| sys/chassis-4/enc-1/disk-29 | HUS726060AL4210 | not-applicable | CHDISK754 |
| sys/chassis-4/enc-1/disk-3 | HUS726060AL4210 | not-applicable | CHDISK728 |
| sys/chassis-4/enc-1/disk-30 | HUS726060AL4210 | not-applicable | CHDISK755 |
| sys/chassis-4/enc-1/disk-31 | HUS726060AL4210 | not-applicable | CHDISK756 |
| sys/chassis-4/enc-1/disk-32 | HUS726060AL4210 | not-applicable | CHDISK757 |
| sys/chassis-4/enc-1/disk-33 | HUS726060AL4210 | not-applicable | CHDISK758 |
| sys/chassis-4/enc-1/disk-34 | HUS726060AL4210 | not-applicable | CHDISK759 |
| sys/chassis-4/enc-1/disk-35 | HUS726060AL4210 | not-applicable | CHDISK760 |
| sys/chassis-4/enc-1/disk-36 | HUS726060AL4210 | not-applicable | CHDISK761 |
| sys/chassis-4/enc-1/disk-37 | HUS726060AL4210 | not-applicable | CHDISK762 |
| sys/chassis-4/enc-1/disk-38 | HUS726060AL4210 | not-applicable | CHDISK763 |
| sys/chassis-4/enc-1/disk-39 | HUS726060AL4210 | not-applicable | CHDISK764 |
| sys/chassis-4/enc-1/disk-4 | HUS726060AL4210 | not-applicable | CHDISK729 |
| sys/chassis-4/enc-1/disk-40 | HUS726060AL4210 | not-applicable | CHDISK765 |
| sys/chassis-4/enc-1/disk-41 | HUS726060AL4210 | not-applicable | CHDISK766 |
| sys/chassis-4/enc-1/disk-42 | HUS726060AL4210 | not-applicable | CHDISK767 |
| sys/chassis-4/enc-1/disk-43 | HUS726060AL4210 | not-applicable | CHDISK768 |
| sys/chassis-4/enc-1/disk-44 | HUS726060AL4210 | not-applicable | CHDISK769 |
| sys/chassis-4/enc-1/disk-45 | HUS726060AL4210 | not-applicable | CHDISK770 |
| sys/chassis-4/enc-1/disk-46 | HUS726060AL4210 | not-applicable | CHDISK771 |
| sys/chassis-4/enc-1/disk-47 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK772 |
| sys/chassis-4/enc-1/disk-48 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK773 |
| sys/chassis-4/enc-1/disk-49 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK774 |
| sys/chassis-4/enc-1/disk-5 | HUS726060AL4210 | not-applicable | CHDISK730 |
| sys/chassis-4/enc-1/disk-50 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK775 |
| sys/chassis-4/enc-1/disk-51 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK776 |
| sys/chassis-4/enc-1/disk-52 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK777 |
| sys/chassis-4/enc-1/disk-53 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK778 |
| sys/chassis-4/enc-1/disk-54 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK779 |
| sys/chassis-4/enc-1/disk-55 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK780 |
| sys/chassis-4/enc-1/disk-56 | INTEL SSDSC2BB016T6K1 | not-applicable | CHDISK781 |
| sys/chassis-4/enc-1/disk-6 | HUS726060AL4210 | not-applicable | CHDISK731 |
| sys/chassis-4/enc-1/disk-7 | HUS726060AL4210 | not-applicable | CHDISK732 |
| sys/chassis-4/enc-1/disk-8 | HUS726060AL4210 | not-applicable | CHDISK733 |
| sys/chassis-4/enc-1/disk-9 | HUS726060AL4210 | not-applicable | CHDISK734 |

## 2.2 Fabric Interconnects

| Relative Name | IP Address | Subnet Mask | Deafult Gateway | MAC Address | Operability | Thermal | Model | Serial |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| switch-A | 192.168.2.116 | 255.255.255.0 | 192.168.2.1 | 00:00:00:00:00:00 | operable | unknown | UCS-FI-6332-16UP | JAB121800UL |
| switch-B | 192.168.2.117 | 255.255.255.0 | 192.168.2.1 | 00:00:00:00:00:00 | operable | unknown | UCS-FI-6332-16UP | JAB221800UL |

## 2.2.1 Fabric Interconnect Modules

| Relative Name | Model | Description | Port Count | Operability | State | Power | Serial |
| --- | --- | --- | --- | --- | --- | --- | --- |
| slot-1 | UCS-FI-6332-16UP | Cisco UCS 6332-16UP 40 Port 1RU Fabric Interconne | 40 | operable | on | on | JAB121800UL |
| slot-1 | UCS-FI-6332-16UP | Cisco UCS 6332-16UP 40 Port 1RU Fabric Interconne | 40 | operable | on | on | JAB221800UL |

## 3 Firmware

### 3.1 UCS Manager

| Distinguished Name | Type | Version |
| --- | --- | --- |
| capabilities/ep/mgmt-ext/fw-system | mgmt-ext |  |

### 3.2 Fabric Interconnect

| Distinguished Name | Type | Version |
| --- | --- | --- |
| sys/switch-B/mgmt/fw-kernel | switch-kernel | 5.0(3)N2(2.10.466) |
| sys/switch-A/mgmt/fw-system | switch-software | 5.0(3)N2(2.10.466) |
| sys/switch-A/mgmt/fw-kernel | switch-kernel | 5.0(3)N2(2.10.466) |
| sys/switch-B/mgmt/fw-system | switch-software | 5.0(3)N2(2.10.466) |

### 3.3 IOM

| Deployment | Distinguished Name | Type | Version |
| --- | --- | --- | --- |
| system | sys/chassis-1/slot-1/mgmt/fw-system | iocard | 3.1(1e) |
| system | sys/chassis-1/slot-2/mgmt/fw-system | iocard | 3.1(1e) |
| system | sys/chassis-3/slot-1/mgmt/fw-system | iocard | 3.1(1e) |
| system | sys/chassis-3/slot-2/mgmt/fw-system | iocard | 3.1(1e) |

### 3.4 Server Adapters

| Deployment | Distinguished Name | Type | Version |
| --- | --- | --- | --- |
| system | sys/chassis-1/blade-1/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-1/blade-2/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-1/blade-3/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-1/blade-4/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-1/blade-5/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-1/blade-6/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-1/blade-7/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-1/blade-8/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-2/slot-1/shared-io-module/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-2/slot-2/shared-io-module/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-3/blade-1/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-3/blade-2/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-3/blade-3/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-3/blade-4/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-3/blade-5/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-3/blade-6/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-3/blade-7/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-3/blade-8/adaptor-1/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-4/slot-1/shared-io-module/mgmt/fw-system | adaptor | 3.2(3e) |
| system | sys/chassis-4/slot-2/shared-io-module/mgmt/fw-system | adaptor | 3.2(3e) |

### 3.5 Server CIMC

| Deployment | Distinguished Name | Type | Version |
| --- | --- | --- | --- |
| system | sys/chassis-1/blade-1/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-1/blade-2/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-1/blade-3/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-1/blade-4/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-1/blade-5/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-1/blade-6/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-1/blade-7/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-1/blade-8/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-2/blade-1/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-2/blade-2/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-3/blade-1/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-3/blade-2/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-3/blade-3/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-3/blade-4/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-3/blade-5/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-3/blade-6/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-3/blade-7/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-3/blade-8/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-4/blade-1/mgmt/fw-system | blade-controller | 3.1(1e) |
| system | sys/chassis-4/blade-2/mgmt/fw-system | blade-controller | 3.1(1e) |

### 3.6 Server BIOS

| Distinguished Name | Type | Version |
| --- | --- | --- |
| sys/chassis-1/blade-1/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-1/blade-2/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-1/blade-3/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-1/blade-4/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-1/blade-5/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-1/blade-6/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-1/blade-7/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-1/blade-8/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-2/blade-1/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-2/blade-2/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-3/blade-1/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-3/blade-2/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-3/blade-3/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-3/blade-4/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-3/blade-5/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-3/blade-6/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-3/blade-7/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-3/blade-8/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-4/blade-1/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |
| sys/chassis-4/blade-2/bios/fw-boot-loader | blade-bios | B00.3.1.1.1.477390817263 |

### 3.7 Host Firmware Packages

| Distinguished Name | Name | Blade Bundle Version | Rack Bundle Version |
| --- | --- | --- | --- |
| org-root/fw-host-pack-default | default |  |  |

# 4 Servers

## 4.1 Service Profiles

## 4.2 Service Profile Templates

### 4.3 Service Profile vNIC Placements

### 4.4 Ethernet VLAN to vNIC Mappings

## 4.5 Policies

### 4.5.1 Maintenance Policies

| Name | Distinguished Name | UptimeDisr | Descr |
| --- | --- | --- | --- |
| default | org-root/maint-default | immediate |  |

### 4.5.2 Boot Policies

| Distinguished Name | Name | Purpose | RebootOnUpdate |
| --- | --- | --- | --- |
| org-root/boot-policy-default | default | operational | no |
| org-root/boot-policy-diag | diag | utility | no |
| org-root/boot-policy-utility | utility | utility | no |

### 4.5.3 SAN Boot Policies

### 4.5.4 Local Disk Policies

| Distinguished Name | Name | Mode | Descr |
| --- | --- | --- | --- |
| org-root/local-disk-config-default | default | any-configuration |  |

### 4.5.5 Scrub Policies

| Distinguished Name | Name | BiosSettingsScrub | DiskScrub |
| --- | --- | --- | --- |
| org-root/scrub-default | default | no | no |

### 4.5.6 BIOS Policies

| Distinguished Name | Name |
| --- | --- |
| org-root/bios-prof-usNIC | usNIC |

#### 4.5.6.1 BIOS Policy Settings

| Distinguished Name | VpQuietBoot |
| --- | --- |
| org-root/bios-prof-usNIC/Quiet-Boot | platform-default |

| Distinguished Name | VpPOSTErrorPause |
| --- | --- |
| org-root/bios-prof-usNIC/POST-error-pause | platform-default |

| Distinguished Name | VpResumeOnACPowerLoss |
| --- | --- |
| org-root/bios-prof-usNIC/Resume-on-AC-power-loss | platform-default |

| Distinguished Name | VpFrontPanelLockout |
| --- | --- |
| org-root/bios-prof-usNIC/Front-panel-lockout | platform-default |

| Distinguished Name | VpIntelTurboBoostTech |
| --- | --- |
| org-root/bios-prof-usNIC/Intel-Turbo-Boost-Tech | enabled |

| Distinguished Name | VpEnhancedIntelSpeedStepTech |
| --- | --- |
| org-root/bios-prof-usNIC/Enhanced-Intel-SpeedStep-Tech | enabled |

| Distinguished Name | VpIntelHyperThreadingTech |
| --- | --- |
| org-root/bios-prof-usNIC/Intel-HyperThreading-Tech | disabled |

| Distinguished Name | VpCoreMultiProcessing |
| --- | --- |
| org-root/bios-prof-usNIC/Core-MultiProcessing | all |

| Distinguished Name | VpExecuteDisableBit |
| --- | --- |
| org-root/bios-prof-usNIC/Execute-Disable-Bit | disabled |

| Distinguished Name | VpIntelVirtualizationTechnology |
| --- | --- |
| org-root/bios-prof-usNIC/Intel-Virtualization-Technology | enabled |

| Distinguished Name | VpDirectCacheAccess |
| --- | --- |
| org-root/bios-prof-usNIC/Direct-Cache-Access | enabled |

| Distinguished Name | VpProcessorCState |
| --- | --- |
| org-root/bios-prof-usNIC/Processor-C-State | platform-default |

| Distinguished Name | VpProcessorC1E |
| --- | --- |
| org-root/bios-prof-usNIC/Processor-C1E | disabled |

| Distinguished Name | VpProcessorC3Report |
| --- | --- |
| org-root/bios-prof-usNIC/Processor-C3-Report | platform-default |

| Distinguished Name | VpProcessorC6Report |
| --- | --- |
| org-root/bios-prof-usNIC/Processor-C6-Report | disabled |

| Distinguished Name | VpProcessorC7Report |
| --- | --- |
| org-root/bios-prof-usNIC/Processor-C7-Report | platform-default |

| Distinguished Name | VpCPUPerformance |
| --- | --- |
| org-root/bios-prof-usNIC/CPU-Performance | platform-default |

| Distinguished Name | VpProcessorMtrr |
| --- | --- |
| org-root/bios-prof-usNIC/Max-Variable-MTRR-Setting | platform-default |

| Distinguished Name | VpIntelVTDATSSupport | VpIntelVTDCoherencySupport | VpIntelVTDInterruptRemapping | VpIntelVTDPassThroughDMASupport | VpIntelVTForDirectedIO |
| --- | --- | --- | --- | --- | --- |
| org-root/bios-prof-usNIC/Intel-VT-for-directed-IO | enabled | enabled | platform-default | platform-default | enabled |

| Distinguished Name | VpSelectMemoryRASConfiguration |
| --- | --- |
| org-root/bios-prof-usNIC/SelectMemory-RAS-configuration | maximum-performance |

| Distinguished Name | VpNUMAOptimized |
| --- | --- |
| org-root/bios-prof-usNIC/NUMA-optimized | enabled |

| Distinguished Name | VpLvDDRMode |
| --- | --- |
| org-root/bios-prof-usNIC/LvDIMM-Support | performance-mode |

| Distinguished Name | VpLegacyUSBSupport | VpMakeDeviceNonBootable |
| --- | --- | --- |
| org-root/bios-prof-usNIC/USB-Boot-Config | platform-default | platform-default |

| Distinguished Name | VpUSBFrontPanelLock |
| --- | --- |
| org-root/bios-prof-usNIC/USB-Front-Panel-Access-Lock | platform-default |

| Distinguished Name | VpUSBIdlePowerOptimizing |
| --- | --- |
| org-root/bios-prof-usNIC/USB-System-Idle-Power-Optimizing-Setting | platform-default |

| Distinguished Name | VpMaximumMemoryBelow4GB |
| --- | --- |
| org-root/bios-prof-usNIC/Maximum-memory-below-4GB | platform-default |

| Distinguished Name | VpMemoryMappedIOAbove4GB |
| --- | --- |
| org-root/bios-prof-usNIC/Memory-mapped-IO-above-4GB | disabled |

| Distinguished Name | VpBootOptionRetry |
| --- | --- |
| org-root/bios-prof-usNIC/Boot-option-retry | platform-default |

| Distinguished Name | VpSASRAID | VpSASRAIDModule |
| --- | --- | --- |
| org-root/bios-prof-usNIC/Intel-entry-SAS-RAID-module | platform-default | platform-default |

| Distinguished Name | VpOSBootWatchdogTimer |
| --- | --- |
| org-root/bios-prof-usNIC/OS-Boot-Watchdog-Timer | platform-default |

## 4.6 Pools

### 4.6.1 UUID Pools

| Distinguished Name | Name | AssignmentOrder | Prefix | Size | Assigned |
| --- | --- | --- | --- | --- | --- |
| org-root/uuid-pool-default | default | default | B15F9ADA-9040-11E8 | 0 | 0 |

### 4.6.2 UUID Pool Blocks

### 4.6.3 UUID Pool Assignments

### 4.6.4 Server Pools

| Distinguished Name | Name | Assigned |
| --- | --- | --- |
| org-root/compute-pool-default | default | 0 |

### 4.6.5 Server Pool Assignments

# 5 LAN

## 5.1 LAN Cloud

## 5.1.1 Fabric Interconnect Ethernet Switching Mode

| Rn | Mode |
| --- | --- |
| lan | end-host |

## 5.1.2 Fabric Interconnect Ethernet Port Configuration

| Distinguished Name | IfRole | LicState | Mode | OperState | OperSpeed | XcvrType |
| --- | --- | --- | --- | --- | --- | --- |
| sys/switch-A/slot-1/switch-ether/port-17 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-A/slot-1/switch-ether/port-18 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-A/slot-1/switch-ether/port-19 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-A/slot-1/switch-ether/port-20 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-A/slot-1/switch-ether/port-21 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-A/slot-1/switch-ether/port-22 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-A/slot-1/switch-ether/port-23 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-A/slot-1/switch-ether/port-24 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-A/slot-1/switch-ether/port-25 | server | license-ok | fabric | up | 10gbps | unknown |
| sys/switch-A/slot-1/switch-ether/port-26 | server | license-ok | fabric | up | 10gbps | unknown |
| sys/switch-A/slot-1/switch-ether/port-27 | server | license-ok | fabric | up | 10gbps | unknown |
| sys/switch-A/slot-1/switch-ether/port-28 | server | license-ok | fabric | up | 10gbps | unknown |
| sys/switch-B/slot-1/switch-ether/port-17 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-B/slot-1/switch-ether/port-18 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-B/slot-1/switch-ether/port-19 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-B/slot-1/switch-ether/port-20 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-B/slot-1/switch-ether/port-21 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-B/slot-1/switch-ether/port-22 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-B/slot-1/switch-ether/port-23 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-B/slot-1/switch-ether/port-24 | server | license-graceperiod | fabric | up | 10gbps | unknown |
| sys/switch-B/slot-1/switch-ether/port-25 | server | license-ok | fabric | up | 10gbps | unknown |
| sys/switch-B/slot-1/switch-ether/port-26 | server | license-ok | fabric | up | 10gbps | unknown |
| sys/switch-B/slot-1/switch-ether/port-27 | server | license-ok | fabric | up | 10gbps | unknown |
| sys/switch-B/slot-1/switch-ether/port-28 | server | license-ok | fabric | up | 10gbps | unknown |

## 5.1.3 Fabric Interconnect Ethernet Uplink Port Channels

## 5.1.4 Fabric Interconnect Ethernet Uplink Port Channel Member

## 5.1.5 QoS System Class Configuration

| Priority | AdminState | Cos | Weight | Drop | Mtu |
| --- | --- | --- | --- | --- | --- |
| bronze | disabled | 1 | 7 | drop | normal |
| gold | disabled | 4 | 9 | drop | normal |
| platinum | disabled | 5 | 10 | no-drop | normal |
| silver | disabled | 2 | 8 | drop | normal |

## 5.1.6 Ethernet VLANs

## 5.2 Policies

### 5.2.1 QoS Policies

### 5.2.2 QoS vNIC Policy Map

### 5.2.3 Network Control Policies

| Distinguished Name | Name | Cdp | UplinkFailAction |
| --- | --- | --- | --- |
| fabric/eth-estc/nwctrl-default | default | disabled | link-down |
| org-root/nwctrl-default | default | disabled | link-down |

### 5.2.4 vNIC Templates

### 5.2.5 Ethernet VLAN to vNIC Mappings

## 5.3 Pools

### 5.3.1 IP Pools

| Distinguished Name | Name | AssignmentOrder | Size |
| --- | --- | --- | --- |
| org-root/ip-pool-ext-mgmt | ext-mgmt | default | 0 |
| org-root/ip-pool-iscsi-initiator-pool | iscsi-initiator-pool | default | 0 |

### 5.3.2 IP Pool Blocks

### 5.3.3 CIMC IP Pool Assignments

### 5.3.4 MAC Address Pools

| Distinguished Name | Name | AssignmentOrder | Size | Assigned |
| --- | --- | --- | --- | --- |
| org-root/mac-pool-default | default | default | 0 | 0 |

### 5.3.5 MAC Address Pool Blocks

### 5.3.6 MAC Address Pool Assignments

# 6 SAN

## 6.1 SAN Cloud

### 6.1.1 Fabric Interconnect Fibre Channel Switching Mode

| Rn | Mode |
| --- | --- |
| san | end-host |

### 6.1.2 Fabric Interconnect FC Uplink Ports

### 6.1.3 Fabric Interconnect FC Uplink Port Channels

### 6.1.4 Fabric Interconnect FCoE Uplink Ports

### 6.1.5 Fabric Interconnect FCoE Uplink Port Channels